/*User defines the input parameters here.*/
/*Note: sigma and b are strictly greater than zero*/
/*Do not modify the format.*/
/*-------------------------------*/

/*int LengthTimes : number of times for the inversion*/
16

/*precReal *Timevec times for the inversions */
0.25 0.5 0.75 1.0 1.25 1.5 1.75 2.0 2.25 2.5 2.75 3.0 3.25 3.5 3.75 4.0

/*precReal *RelErrorTol : relative error tolerance for the inversions */
0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01 0.01

/*int SearchSwitch : 1-search for parameters, 0-user defined paramters*/
1

/*int LengthLag : number of Laguerre coefficients used in the search*/
1

/*int *NLag : default number of Laguerre expansion coefficients*/
16

/*Used if and only if SearchSwitch = 0--------------------------------------------------------------*/

/*precReal sigmaUser : sigma user defined value for each time*/
1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 1.0 

/*precReal bUser : b user defined value for each time*/
4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 4.0 

/*Used if and only if SearchSwitch = 1, default values are often sufficient-------------------------*/

/*int Lengthtol : length of the tolerances searched 3*/
1

/*precReal sigmin : minimum sigma value searched*/
0.0

/*precReal sigmax : maximum sigma value searched*/
20.0 

/*precReal *tols : sigma grid resolution*/
0.25

/*precReal bmax : maximum b value searched*/
40.0

/*precReal *tolb : b grid resolution*/
0.25