/*User defines the input parameters here.*/
/*Note: sigma and b are strictly greater than zero*/
/*Do not modify the format.*/
/*-------------------------------*/

/*int LengthTimes : number of times for the inversion*/
3

/*precReal *Timevec times for the inversions */
0.5 0.75 1.0

/*precReal *RelErrorTol : relative error tolerance for the inversions */
0.01 0.01 0.01

/*int SearchSwitch : 1-search for parameters, 0-user defined paramters*/
1

/*int LengthLag : number of Laguerre coefficients used in the search*/
3

/*int *NLag : default number of Laguerre expansion coefficients*/
16 32 64

/*Used if and only if SearchSwitch = 0--------------------------------------------------------------*/

/*precReal sigmaUser : sigma user defined value for each time*/
1.0 1.0 1.0

/*precReal bUser : b user defined value for each time*/
4.0 4.0 4.0

/*Used if and only if SearchSwitch = 1, default values are often sufficient-------------------------*/

/*int Lengthtol : length of the tolerances searched 3*/
3

/*precReal sigmin : minimum sigma value searched*/
0

/*precReal sigmax : maximum sigma value searched*/
20.0 

/*precReal *tols : sigma grid resolution*/
1.0 0.5 0.25

/*precReal bmax : maximum b value searched*/
40.0

/*precReal *tolb : b grid resolution*/
1.0 0.5 0.25
