/*User defines the input parameters here.*/
/*Note: sigma and b are strictly greater than zero*/
/*Do not modify the format.*/
/*-------------------------------*/

/*int LengthTimes : number of times for the inversion*/
1

/*precReal *Timevec times for the inversions */
2.0

/*precReal *RelErrorTol : relative error tolerance for the inversions */
0.01

/*int SearchSwitch : 1-search for parameters, 0-user defined paramters*/
1

/*int LengthLag : number of Laguerre coefficients used in the search*/
1

/*int *NLag : default number of Laguerre expansion coefficients  128 256 512*/
64

/*Used if and only if SearchSwitch = 0--------------------------------------------------------------*/

/*precReal sigmaUser : sigma user defined value for each time*/
1.0

/*precReal bUser : b user defined value for each time*/
4.0

/*Used if and only if SearchSwitch = 1, default values are often sufficient-------------------------*/

/*int Lengthtol : length of the tolerances searched 3*/
1

/*precReal sigmin : minimum sigma value searched*/
0.125

/*precReal sigmax : maximum sigma value searched 20*/
20.0

/*precReal *tols : sigma grid resolution 1.0 0.5 0.25*/
0.125

/*precReal bmax : maximum b value searched 40*/
40.0

/*precReal *tolb : b grid resolution 1.0 0.5 0.25*/
1.0
